and

or and

FF EN

FF FD and

Disc

FF DT LF

FF FC

120 ns

480 ns

960 ns

FC GATE Disc

Disc

Downscale n=100 and

and and

LF

Disc

LF

IOL

Start

JOPL+Start ZDO+Start Teles+Start Start

NO FC Siz1 CsIz1 Siz2 CsIz2 Si-Array ZDO

Techno Cat-Puls GSI-Puls MSU-Puls Tel-Puls TOF-Laser Pedestal Spill on Spill off

FC Siz1 CsIz1 Siz2 CsIz2 Teles Siz2 CsIz2

Disc

Delayed ZDO

Delayed Start TDC

LF

or or

or or TOF

downscaled

TB inh

TB inh

TB inh

MASTER

end

S

R=Clear

R=Clear

S

R=Clear

1-1/n

1-1/n

Deadtime

out out Clear

TBInh end

Reset Set

instant busy out 70μ

8μ

8.4μ

3.2μ

165n

170n

8μ

20μ

500n 8μ

8.5μ

8μ 500n 50n

50n

50μ

Width after Master